WonderSwan Total Sound Driver
Top＼ MML Compiler＼ MML Reference

## MML Reference - Mode switch (PCM) / Dumper switch (MIDI)

PCM : Mode switch of the WonderSwan PCM.
MIDI : Send the Hold(Dumper pedal, Sustain) (Control Change No.64)

### Format

Ps

### Input

Input | Range | Default |
--- | --- | --- | ---
s | 0 to 1 | - | 0:Disable / 1:Enable

### Explanation

If setting channel is MIDI, this command can send the Hold(Dumper pedal, Sustain) of the Control Change No.64.
If setting channel is PCM, this command can set the following mode of the WonderSwan PCM.

Channel | mode
--- | ---
0 to 15 | Hold(Dumper pedal, Sustain) switch of the MIDI
128 | This channel have not mode.
129 | This channel have not mode.
130 | Sweep mode of the WonderSwan PCM channel 3
131 | Noise mode of the WonderSwan PCM channel 4