;English text define table.
;I Infomational Message
;E Error Message
;Translation by Chromaryu. (aka くろま)

;mvc.cs 0000
E0000=Illegal option.
I0000=\r\nPart  Chip    Count
I0001=--------------------
I0002= {0}   {1}   {2}
I0003=\r\nResult
I0004= Warning : (F:{0} L:{1}){2}
I0005= Error : (F:{0} L:{1}){2}
I0006= Errors : {0}\r\n Warnings : {1}
I0007= Loop Clocks  : {0}
I0008= Loop Samples : {0:0.00}({1:0.00}s)
I0009= Total Clocks  : {0}
I0010= Total Samples : {0:0.00}({1:0.00}s)
I0020= ADPCM Data size(YM2608)  : ({0}/262143) bytes
I0021= ADPCM Data size(YM2608Secondary)  : ({0}/262143) bytes
I0022= ADPCM-A Data size(YM2610B)  : ({0}/16777215) bytes
I0023= ADPCM-B Data size(YM2610B)  : ({0}/16777215) bytes
I0024= ADPCM-A Data size(YM2610BSecondary)  : ({0}/16777215) bytes
I0025= ADPCM-B Data size(YM2610BSecondary)  : ({0}/16777215) bytes
I0026= PCM Data size(YM2612)  : {0} bytes
I0027= PCM Data size(RF5C164) : ({0}/65535) bytes
I0028= PCM Data size(RF5C164Secondary) : ({0}/65535) bytes
I0029= PCM Data size(HuC6280)  : {0} bytes
I0030= PCM Data size(HuC6280Secondary)  : {0} bytes
I0031= ADPCM-A Data size(YM2609)  : ({0}/262143) byte
I0032= ADPCM-B Data size(YM2609)  : ({0}/16777215) byte
I0033= ADPCM-C Data size(YM2609)  : ({0}/16777215) byte
I0034= ADPCM-A Data size(YM2609Secondary)  : ({0}/262143) byte
I0035= ADPCM-B Data size(YM2609Secondary)  : ({0}/16777215) byte
I0036= ADPCM-C Data size(YM2609Secondary)  : ({0}/16777215) byte
I0050=\r\nFinished.\r\n



;frmMain 0100
I0100=Compile
I0101=\r\n------------------\r\n
I0102=Start.\r\n
I0103=.gwi File(*.gwi)|*.gwi|All Files.(*.*)|*.*
I0104=Select .gwi file.
I0105=\r\nFinished.\r\n\r\n
I0106=Done.
I0107=\r\nResult\r\n
I0108= Warning : (F:{0} L:{1}){2}\r\n
I0109= Error : (F:{0} L:{1}){2}\r\n
I0110= Errors : {0}\r\n Warnings : {1}\r\n
I0111= Loop  Clocks  : {0}\r\n
I0112= Loop  Samples : {0:0.00}({1:0.00}s)\r\n
I0113= Total Clocks  : {0}\r\n
I0114= Total Samples : {0:0.00}({1:0.00}s)\r\n
I0115= ADPCM Data size(YM2608)              : ({0}/262143) bytes\r\n
I0116= ADPCM Data size(YM2608Secondary)     : ({0}/262143) bytes\r\n
I0117= ADPCM-A Data size(YM2610B)           : ({0}/16777215) bytes\r\n
I0118= ADPCM-B Data size(YM2610B)           : ({0}/16777215) bytes\r\n
I0119= ADPCM-A Data size(YM2610BSecondary)  : ({0}/16777215) bytes\r\n
I0120= ADPCM-B Data size(YM2610BSecondary)  : ({0}/16777215) bytes\r\n
I0121= PCM Data size(YM2612)                : {0} bytes\r\n
I0122= PCM Data size(RF5C164)               : ({0}/65535) bytes\r\n
I0123= PCM Data size(RF5C164Secondary)      : ({0}/65535) bytes\r\n
I0124= PCM Data size(HuC6280)               : {0} bytes\r\n
I0125= PCM Data size(HuC6280Secondary)      : {0} bytes\r\n
I0126=\r\nFinished.\r\n\r\n

E0100=Failed to launch player.
E0101=The acceptable text files must have a .gwi extension.
E0102=The dropped file contains files that do not have a .gwi extension.



;clsVgm.cs 01000
E01000=Ignoring data on undefined part ({0}).
E01001=Recieved empty sound patch definition.
E01002=Selected undefined/unuse ChipName or chip can't use PCM.({0})
E01003=Illegal PCM sound patch definition line.
E01004=Selected unsupported chip of the envelope. / Defined the unused chip envelope.
E01005=Illegal Envelope definition line.
E01006=Illegal ToneDoubler definition.
E01007=Envelope volume is exceeding {0}.
E01008=Envelope volume is below {0}.
E01009=Illegal alias definition.
E01010=Data not found in alias. 
E01011=Illegal part defined.
E01012=Found illegal note patch defintion.
E01013=Illegal WaveForm Sound patch definition.
E01014=ToneDoubler definition illegal.
E01015=Exceeding byte limit (256bytes) per one frame. Please spread datas. Frame {0} : {1}bytes
E01016=Found unknown command {0}.
E01017=Can't define PCM other than YM2612X(OPN2X) on XGM format.
E01018=Failed to load MUCOM88 voice file.
E01019=Failed to load MUCOM88 ADPCM file.
E01020=Found unknown command {0}.(XGM format)
E01021=Failed to load TFI voice file.
E01022=The {0} definition has been truncated in the middle.
E01023=Illegal {0} definition.
E01024=The number of definitions exceeding the default size was detected.(Please also check the number of elements in the definition statement in the foreground.)


;Common.cs 02000
E02000=Failed to load PCM file. (filename:{0})
E02001=PCM File: Illegal RIFF header. (File size below 4B)
E02002=PCM File: Illegal RIFF header. (RIFF)
E02003=PCM File: Illegal RIFF header. (WAVE)
E02004=PCM File: Invalid format ({0})
E02005=PCM File: Channel number ({0}) is different from spec(mono/1ch). 
E02006=PCM File: Sampling rate ({0}) is different from spec(8000/14000/16000/18500).
E02007=PCM File: Bit number per 1 sample ({0}) is different from spec(8bit/16bit).
E02008=PCM File: Invalid data block size. ({0})
E02009=PCM File: File have Invalid or Unknown chunks. ({0})
E02010=Invalid part definition. ({0})



;Information.cs 03000
E03000=Invalid definition. ({0})


;mml2vgm.cs 04000
I04000=Start {0} core
I04001= File existence check
I04002= Get source file
I04003= Parse text
I04004= check PCM definition and get
I04005= MML syntax parsing
I04006= Start VGM_GetByteData
I04007= End   VGM_GetByteData
I04008= Start XGM_GetByteData
I04009= End   XGM_GetByteData
I04010= File Output
I04011=End mml2vgm core
I04012=MODE:\r\n SegaPCM: None\r\n C140:    0=8bit 1=13bit(Compressed 8bit)\r\n
I04013=STATUS:\r\n USED: USED in song\r\n NONE: Not Used in song\r\n Error: Invalid Parameter?\r\n
I04014=C140 PRI : SYSTEM2{0}
I04015=C140 SEC : SYSTEM2{0}
I04016=-- SAMPLE LIST --
I04017=CHIP       PRI/SEC SMPID BANK START(H) END(H)   LOOP(H)  LENGTH(H) MODE STATUS
I04018= Total Length : {0} byte\r\n
I04019=-- DATA BLOCK LIST --
I04020=CHIP       PRI/SEC START(H) END(H)   LENGTH(H) STATUS
I04021=Write VGZ file.
I04022=Write TraceInfo(.ti) file.
I04023= Start ZGM_GetByteData
I04024= End   ZGM_GetByteData
I04025=Write ZGM file.
I04026= Start XGM2_GetByteData
I04027= End   XGM2_GetByteData
I04028=Write XGM2 file.

E04000=File not found.
E04001=Unexpected Error: Failed to get source file.
E04002=Unexpected Error: Failed to parse source(analyze)(line:{0})
E04003=Unexpected Error: MML Parse failed?(MMLAnalyze)(line:{0})
E04004=Unexpected Error: Source analysis failed?(getByteData)(line:{0})
E04005=Unexpected Error: line:{0}\r\nMessage:\r\n{1}\r\nStack Trace:\r\n{2}\r\n
E04006=Include file({0}) not found.
E04007=Failed to load PCM file. (filename:{0})
E04008=Out of memory.


;MMLAnalyze.cs 05000
E05000=Found unknown command {0}.
E05001=Wrong tempo defined.
E05002=Invalid sound patch number defined.
E05003=Invalid volume defined.
E05004=Invalid volume defined.
E05005=Invalid octave defined.
E05006=Invalid volume ')' defined.
E05007=Invalud volume '(' defined.
E05008=Found note length({0}) that isn't dividable. Length will be unstable.
E05009=Invalid note length defined.
E05010=Invalid pan 'p' defined.
E05011=Invalid Detune 'D' defined.
E05012=Invalid PCM Mode selection 'm' selected.
E05013=Invalid gate time selection 'q' selected.
E05014=Invalid gate time selection 'Q' selected.
E05015=Unknown command ('EO{0}') defined.
E05016=Unknown command ('EHO{0}') defined.
E05017=Failed to parse 'EHT' command.
E05018=Failed to parse 'EHT' command.
E05019=Unknown command ('EXO{0}') defined.
E05020=Failed to parse 'EXD' command.
E05021=Invalid slot definition 'EX' defined.
E05022=Failed to parse 'E' command.
E05023=Found note length({0}) that isn't dividable, Length will be unstable.
E05024=Illegal number defined in 'MAMS' command.
E05025=Syntax Error on 'MAMS'.
E05026=LFO channel definable is 'P','Q','R','S'; 4 types only.
E05027=Illegal number defined as 'MPMS' configuration.
E05028='MPMS' Syntax Error.
E05029=LFO channel definable is 'T','V','H','W'; 3 types only.
E05030=Invalid number defined as LFO configuration.
E05031=LFO channel definable is 'P','Q','R','S'; 4 types only.
E05032=Invalid number defined as LFO configuration.
E05033=Invalid number defined as 'w' command.
E05034=Invalid number defined as 'P' command.
E05035=Invalid number defined as 'K' command.
E05036=Found undiviable '.' definition; Note length is unstable.
E05037=before ',','0' commands (ToneDoubler) must be note command.
E05038=Found command unplaceable before ',','0' command (ToneDoubler).
E05039=before '_' command must be note command or ToneDoubler command.
E05040=Found unplaceable command after '_'.
E05041=command must be note or ToneDoubler command before '^'.
E05042=Note or rest command is not found before '^'.
E05043=Must be note or ToneDoubler command before '~'.
E05044=Note or rest command is not found before '~'.
E05045=Must be note or ToneDoubler command before '&'.
E05046=Note command not found before '&'.
E05047=']' not found as escape point from '/'.
E05048=Loop left open. '[' or ']' missing in loop defintion.
E05049=Tuplet and repeat command can't straddle each other.
E05050='{' or '}' missing in sound or meta definiton.
E05051=Failed to parse 'so' or 'sf' command.
E05052=Illegal number defined as 'A' configuration.
E05053=Unknown command ('mo?') defined.
E05054=Unknown command ('DO?') defined.
E05055=Failed to parse 'CH' command.
E05056=Failed to parse 'U' command.
E05057=Failed to parse 'CC' command.
E05058=Invalid number defined as 'wf' command.
E05059=Failed to parse 'X' command.
E05060=Failed to parse '*' command.
E05061=Failed to syncronize '*S' command.
E05062=Unknown command ('APO?') defined.
E05063=Unknown command ('AP?') defined.
E05064=Unknown command ('PRO?') defined.
E05065=Unknown command ('F?') defined.
E05066=Unknown command ('CAO?') defined.
E05067=Unknown command ('CA?') defined.
E05068=Unknown command ('SX?') defined.
E05069=Unknown command ('PDO?') defined.
E05070=Unknown command ('H?') defined.
E05071=Unknown command ('HSO?') defined.
E05072=Unknown command ('HST?') defined.
E05073=Unknown command ('PRV?') defined.
E05074=Unknown command ('FM?') defined.
E05075=Unknown command ('PC?') defined.
E05076=Illegal number defined as '\' configuration.
E05077=Unknown command ('POS?') defined.
E05078=Unknown command ('POR?') defined.
E05079=Unknown command ('POL?') defined.
E05080=Unknown command ('PO?') defined.
E05081='[|' cannot be nested.
E05082=A '|' has been specified even though you have not started a part-wise replacement.
E05083=A '|]' has been specified even though you have not started a part-wise replacement.
E05084=The other cannot be executed during part replacement or part arpeggio.
E05085=Unknown command ('TTO?') defined.
E05086=Unknown command ('VOP?') defined.
E05087=Unknown command ('TLOFS?') defined.
E05088=A slot number is specified that cannot be used. slot enumerates the number of slots (1-4) to be used.
E05089=The value exceeds the range of values that can be specified.
E05090=Unknown command ('VGO?') defined.
E05091=Unknown command ('y') defined.
E05092=Invalid number defined as 'PP' command.


;partWork.cs 06000
E06000=Selected alias is not defined.


;usage 07000
I07000=mml2vgm Commandline Version\r\n                                   By kuma\r\n\r\nUsage:\r\n    mvc gwi[.gwi] [vgm[.vgm|.vgz|.xgm]]\r\n\r\nParameters\r\n   gwi        Please select gwi file.        \r\n               .gwi is autocollected if not specified.\r\n    vgm        can select vgm,vgz,xgm file.              \r\n               You need to define when you're using vgz.      \r\n


;AY8910.cs 08000
E08000=This sound chip doesn't have instruments.
E08001=ToneDoubler cannot be used if chip is not OPN or OPM.
E08002=Sound patch does not exist as PCM definition({0}).
E08003=Selected Tone number({0}) is not for AY8910 PCM data.
E08004=AY8910 can't use PD command.

;C140.cs 09000
E09000=defined loop address [{0}] is exceeding PCM data size. select between 0~{1}.
E09001=This sound chip doesn't have instruments.
E09002=ToneDoubler cannot be used if chip is not OPN or OPM.
E09003=Tone number({0}) does not exist for PCM definition.
E09004=Selected Tone number({0}) is not for C140 PCM data.


;clsChip.cs 10000
E10000=Sound patch selected as envelope definition does not exist.
E10001=Defined LFO parameter is not defined.
E10002=This channel can't use w command.
E10003=This channel can't use MPMS command.
E10004=This channel can't use MAMS command.
E10005=Parameters missing or not enough to setup LFO.
E10006=Parameters number exceeded to setup LFO.
E10007=This channel can't use MPMS command.
E10008=This channel can't use p command.
E10009=This channel can't use m command.
E10010=Envelope analysis failed.
E10011=This channel can't use MH command.
E10012=This part is not eligible for SFX part. ignoring E command.
E10013=Negative note length selected.
E10014=This channel can't use P command.
E10015=This chip can't use P command.
E10016=This chip can't use PD command.
E10017=This chip can't use PI command.
E10018={0} can't use PI command.
E10019=This soundchip doesn't have instruments.
E10020=ToneDoubler cannot be used if chip is not OPN or OPM.
E10021=Selecting undefined sound patch ({0}).
E10022=This channel can't use so or sf command.
E10023=This channel can't use mon or mof command.
E10024=This PCM map No({0}) is not defined.
E10025=This Note(o{0}{1} shift:{2}) is not defined.
E10026=This channel can't use V command.
E10027=This channel can't use DOF or DON command.
E10028=This channel can't use CH command.
E10029=This channel can't use U command.
E10030=Sound patch isn't selected.
E10031=This channel can't use CC command.
E10032=This channel can't use wf command.
E10033=This channel can't use X command.
E10034=Arpeggio analysis failed.
E10035=This channel can't use F command.
E10036=Command Arpeggio analysis failed.
E10037=Selecting undefined VolumeArpeggio.
E10038=An undefined number was specified. or VolumeArpeggio enabled without specification.
E10039=Selecting undefined Arpeggio.
E10040=An undefined number was specified. or Arpeggio enabled without specification.
E10041=Selecting undefined CommandArpeggio.
E10042=An undefined number was specified. or CommandArpeggio enabled without specification.
E10043=This channel can't use KD command.
E10044=This channel can't use HS command.
E10045=This channel can't use PRV command.
E10046=This channel can't use FM command.
E10047=Use the POx command to initialize the system before using the __ command.
E10048=This channel can't use TTON/TTOF command.
E10049=This chip can't use VOP command.
E10050=This chip can't use VGON/VGOF command.


;clsOPN.cs 11000
E11000=Can't change volume if defined note patch ({0}) is undefined.
E11001=Selected undefined note patch ({0}).
E11002=Can't change sound patch in extended channels.
E11003=This soundchip doesn't have instruments.
E11004=Envelope analysis failed.
E11005=Unknown command defined. (EX{0})
E11006=There are 4 | 1 parameters for the KD command.
E11007=A non-numeric value has been specified for the KD command parameter.
E11008=Sound patch does not exist as PCM definition({0}).
E11009=Selected Tone number({0}) is not for {1} PCM data.
E11010=Unknown command defined. (TTON/TTOF)
E11011=The specified value of VOP is invalid.
E11012=Unknown command defined. (TLOFS)
E11013=A slot number is specified that cannot be used. slot enumerates the number of slots (1-4) to be used.
E11014=The tone number specified in the PCM definition has not been specified. Use the @ command to specify it.
E11015=This channel can't use @E command.


;HuC6280.cs 12000
E12000=Selecting undefined sound patch ({0}).
E12001=Parameters missing or not enough to setup LFO.
E12002=Parameters number exceeded to setup LFO.
E12003=This soundchip doesn't have instruments.
E12004=ToneDoubler cannot be used if chip is not OPN or OPM.
E12005=Sound patch does not exist as PCM definition({0}).
E12006=Selected Tone number({0}) is not for HuC6280 PCM data.
E12007=HuC6280 can't use PD command.



;RF5C164.cs 13000
E13001=This soundchip doesn't have instruments.
E13002=ToneDoubler cannot be used if chip is not OPN or OPM.
E13003=Sound patch does not exist as PCM definition({0}).
E13004=Selected Tone number({0}) is not for RF5C164 PCM data.



;segaPcm.cs 14000
E14001=This soundchip doesn't have instruments.
E14002=ToneDoubler cannot be used if chip is not OPN or OPM.
E14003=Sound patch does not exist as PCM definition({0}).
E14004=Selected Tone number({0}) is not for SEGAPCM PCM data.



;SN76489.cs 15000
E15001=This soundchip doesn't have instruments.
E15002=ToneDoubler cannot be used if chip is not OPN or OPM.



;YM2151.cs 16000
E16000=Can't change volume if defined note patch ({0}) is undefined.
E16001=Selected undefined note patch ({0}).
E16002=Parameters missing or not enough to setup LFO.
E16003=Parameters number exceeded to setup LFO.
E16004=Can't select panning before sound patch definition.
E16005=This soundchip doesn't have instruments.



;YM2413.cs 17000
E17000=Selected undefined note patch ({0}).
E17001=ToneDoubler cannot be used if chip is not OPN or OPM.
E17002=Selected Tone number({0}) is not for YM2413 data.



;YM2608.cs 18000
E18000=MPMS command in Non-FM channel will be ignored.
E18001=MAMS command in Non-FM channel will be ignored.
E18002=Parameters missing or not enough to setup LFO.
E18003=Parameters number exceeded to setup LFO.
E18004=Sound patch does not exist as PCM definition({0}).
E18005=Selected Tone number({0}) is not for YM2608 PCM data.



;YM2610B.cs 19000
E19000=MPMS command in Non-FM channel will be ignored.
E19001=MAMS command in Non-FM channel will be ignored.
E19002=Parameters missing or not enough to setup LFO.
E19003=Parameters number exceeded to setup LFO.
E19004=Sound patch does not exist as PCM definition({0}).
E19005=Selected Tone number({0}) is not for YM2610B PCM data.



;YM2612.cs 20000
E20000=Parameters missing or not enough to setup LFO.
E20001=Parameters number exceeded to setup LFO.
E20002=Sound patch does not exist as PCM definition({0}).
E20003=Selected Tone number({0}) is not for YM2612 PCM data.
E20004=YM2612 can't use PD command.



;YM2612X.cs 21000
E21000=Sound patch does not exist as PCM definition({0}).
E21001=Selected Tone number({0}) is not for YM2612-XGM PCM data.


;QSound.cs 22000
E22000=defined loop address [{0}] is exceeding PCM data size. select between 0~{1}.
E22001=This sound chip doesn't have instruments.
E22002=ToneDoubler cannot be used if chip is not OPN or OPM.
E22003=Tone number({0}) does not exist for PCM definition.
E22004=Selected Tone number({0}) is not for QSound PCM data.
E22005=Sound patch isn't selected.


;K053260.cs 23000
E23000=defined loop address [{0}] is exceeding PCM data size. select between 0~{1}.
E23001=This sound chip doesn't have instruments.
E23002=ToneDoubler cannot be used if chip is not OPN or OPM.
E23003=Tone number({0}) does not exist for PCM definition.
E23004=Selected Tone number({0}) is not for K053260 PCM data.
E23005=Sound patch isn't selected.


;SourceParcer.cs 24000
E24000=The number of definitions per sound chip has exceeded the allowable number.(Format:{0} Max:{1} Specify:{2})
E24001=A definition of sound chip({1}) that cannot be used in the {0} format.


;MidiGM.cs 25000
W25000=The target of DirectMode ('V', 'T') is not specified.

;YMF262.cs 26000
E26000=Specified 4operator sound patch({0}) on 2operator channel.
E26001=Specified 2operator sound patch({0}) on 4operator channel.
W26002=Specified command that's only for 4operator channel. Will be ignored.



;C352.cs 27000
E27000=defined loop address [{0}] is exceeding PCM data size. select between 0~{1}.
E27001=This sound chip doesn't have instruments.
E27002=ToneDoubler cannot be used if chip is not OPN or OPM.
E27003=Tone number({0}) does not exist for PCM definition.
E27004=Selected Tone number({0}) is not for C352 PCM data.



;Y8950.cs 28000
E28004=Tone number({0}) does not exist for PCM definition.
E28005=Selected Tone number({0}) is not for Y8950 ADPCM data.
E28006=This sound chip doesn't support 4-operator mode, so L4 format voices cannot be used.



;YM3526.cs 29000
E29006=This sound chip doesn't support 4-operator mode, so L4 format voices cannot be used.



;YM3812.cs 30000
E30006=This sound chip doesn't support 4-operator mode, so L4 format voices cannot be used.




;NES.cs 32000
E32000=Duty cycle can only be used on pulse channels.
E32001=NES can't use PD command.
E32002=Parameters missing or not enough to setup LFO.
E32003=Parameters number exceeded to setup LFO.
E32004=Selecting undefined sound patch ({0}).


;YM2612X2.cs 33000
E33000=Sound patch does not exist as PCM definition({0}).
E33001=Selected Tone number({0}) is not for YM2612-XGM2 PCM data.


