Using expansion chips in PAL mode - FamiTracker

# FamiTracker

FamiTracker Support Forums

Skip to content

## Using expansion chips in PAL mode

General discussion about tracking, help and support.
Post Reply

- Print view

1 post • Page 1 of 1

djmaximum
  Posts: 12
  Joined: Thu May 14, 2015 12:58 am
  Location: NES Gameboy land

### Using expansion chips in PAL mode

- Quote

Post by djmaximum » Tue Jul 25, 2017 6:12 am

So I was playing around with an earlier version of Famitracker and was basically having fun with the MMC5 and VRC6 in PAL mode. What I do know is that the MMC5 is also using PAL pitch table periods, wile the VRC6 literally forces everything to use an NTSC pitch table period in NSF export. Personally it doesn't bother me if my VRC6 NSFs are a semitone lower compared to Famitracker's output.

Attachments
  PAL MMC5 temp.nsf
    Same song but with MMC5
    (17.25 KiB) Downloaded 186 times
  PAL VRC6 temp.nsf
    (17.25 KiB) Downloaded 186 times

Other places where you can find my music.
my chiptune up
my chipmusic
my BOTB
Top

Post Reply

- Print view

1 post • Page 1 of 1

Return to “General Talk”

Jump to

- Rules
- Wiki
- FamiTracker
- General Talk
- Bug Reports
- Feature Requests
- Source and development
- Music
- Original Music
- Cover Music
- Other
- Site Issues & Suggestions